   Workstation for DOS ODI Client

   Introduction:
   -------------
   This document describes the procedure to setup the NetWare v3.X , v4.X
   workstation driver for Unex ND01X Ethernet/Fast Ethernet PCI Bus adapter.

   Location of Driver:  \NWCLIENT\DOS\ND01XODI.COM (diskette) or
                        \DRIVERS\NIC\ND01X\NWCLIENT\DOS\ND01XODI.COM (CD-ROM)

   Sample Configuration Files:
   ---------------------------
     STARTNET.BAT:
         LSL
         ND01XODI
         IPXODI
         NETX or VLM (VLM's for NetWare 4.x )

     NET.CFG:
         LINK DRIVER ND01XODI

         ;  BUSNO NN   --where NN is the PCI bus identifier of the PCI bus
         ;               which connectsto the adapter.
         ;  DEVICENO NN --where NN is the specific PCI BIOS device
         ;                identification number of the specified PCI adapter.
         ; [ or you can use "EtherID" to select a specific ND01X adapter:
         ;  EtherID NNNNNNNNNNNN --Where NNNNNNNNNNNN specify a ND01X
         ;                         adapter's node address.This is only
         ;                         required when more than one ND01X
         ;                         adapters exist on one system.
         ; ]


           FRAME Ethernet_802.2 --Specify frame type
           FRAME Ethernet_802.3
           FRAME Ethernet_SNAP
           FRAME Ethernet_II

         NetWare DOS Requester
           FIRST NETWORK DRIVE = F
           NETWARE PROTOCOL = NDS BIND
         ;  PREFERRED SERVER = NW411


   Setup Procedures for NetWare 3.11/3.12 Client :
   -----------------------------------------------
      Before you start with the installation process, make sure that
      the  adapter is properly installed and configured. Make sure
      that your NetWare workstation is properly installed.

      1. Copy  ND01XODI.COM from the Unex Driver Diskette subdirectory
         A:\NWCLIENT\DOS to your harddisk.

      2. Create a batch file, or add to your STARTNET.BAT file the commands
         listed above under STARTNET.BAT

      3. Edit the NET.CFG file that you copied over. Edit the file per your
         requirements (see examples above).  If there are two frame types
         listed, whichever frame type is listed first, that is the one that
         the  driver will load.  See above for examples.  The NET.CFG file
         should be in the same directory with the LSL.COM file.


   Setup Procedures for NetWare 4.X Client with vlm:
   -----------------------------------------------
      The  installation utility  INSTALL.EXE  is  located on NetWare's
      "Workstation for DOS" disk. Run INSTALL.EXE from the Workstation
      for DOS Disk.

      The NetWare Client Install program screen will appear.  You must
      complete each of the questions.  These options are specific to your
      needs.

      1. Enter the destination directory for the NetWare Client.
         (The default directory is C:\NWCLIENT).

      2. Gives you the option to automatically update the CONFIG.SYS
         and the AUTOEXEC.BAT files or modify them at a later time
         manually.

      3. Do you wish to install support for MS Windows ? (Y/N)
         (MS Windows Subdirectory: default C:\WINDOWS)

      4. Asks you to select a network driver and provide  configuration
         options.  It uses  the specifications you select to create the
         file NET.CFG. Insert the Unex drivers disk when prompted for
         the driver disk and specify the driver path A:\NWCLIENT\DOS

      5. Press <Enter> to install


   NOTE:
   -----
      1. Be sure to add LASTDRIVE=Z to your CONFIG.SYS file for the
         network mappings to work properly.

      2. When you have multiple ND01X Adapters on your system:
         Use "BUSNO" and "DEVICENO" KEYWORD in NET.CFG to select which
         adapter to use with your netware client.(or you can use "EtherID")


                                        -- Unex Technology Corporation --
