   Netware Client32 Driver

   Introduction:
   -------------
   This document describes the procedure to install the NetWare Client32
   driver for Unex ND01X Fast Ethernet adapter.

   Location of Driver:  \CLIENT32\ND01XSRV.LAN (diskette) or
                        \DRIVERS\NIC\ND01X\CLIENT32\ND01XSRV.LAN (CD-ROM)


   Sample Configuration Files:
   ---------------------------
      STARTNET.BAT (Client 32 for DOS will contain):

          C:\NOVELL\CLIENT32\NIOS.EXE
          LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
          LOAD C:\NOVELL\CLIENT32\CMSM.NLM
          LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
          LOAD C:\NOVELL\CLIENT32\ND01XSRV.LAN FRAME=ETHERNET_802.2
          LOAD C:\NOVELL\CLIENT32\ND01XSRV.LAN FRAME=Ethernet_802.3
          LOAD C:\NOVELL\CLIENT32\ND01XSRV.LAN FRAME=Ethernet_II
          LOAD C:\NOVELL\CLIENT32\ND01XSRV.LAN FRAME=Ethernet_SNAP

   A. Driver Installation Procedures on Clien32 for DOS :
   ------------------------------------------------------
     1.If you have completed installed the Netware Client 32 for DOS, all
       you have to do is to modify STARTNET.BAT.  Please see the  sample
       STARTNET.BAT above. If not, Please follow the next step 2 - step 7.

     2.Run INSTALL.EXE from Netware Client 32 for DOS diskette 1 (or from
       Netware 4.11 CD).  When  the  product  manual  appears,  mark the
       "Netware Client 32 for DOS" item, then press <Enter>.

     3.Select "USER SPECIFIED 32 BIT DRIVER" item from "32-bit Network
       Board Drivers" menu, then press <Enter>.

     4.Insert Unex ND01X Driver Diskette, then specify the driver path
       A: or B:

     5.Select "Unex ND01X Fast Ethernet driver", then press <Enter>.

     6.Following instructions to complete the Client32 for DOS software
       installation.

     7.Reboot your machine.

      Installation Notes:
      -------------------
      * Installing Multiple LAN Adapters:
         The keyword  "SLOT"  is provided for multiple LAN adapters in a
         single server by the driver ND01XSRV.LAN. So, add "SLOT" in LOAD
         commands. For example:

         C:\NOVELL\CLIENT32\NIOS.EXE
         LOAD LSLC32.NLM
         LOAD CMSM.NLM
         LOAD ETHERTSM.NLM
         LOAD ND01XSRV FRAME=Ethernet_802.2 SLOT=1
         LOAD ND01XSRV FRAME=Ethernet_802.2 SLOT=2

   B. Driver Installation Procedures on Client32 for Windows 3.x :
   ---------------------------------------------------------------
     Refer to Content A. On step 2, mark "Netware Client 32 for DOS"  and
     "Client 32 for Windows".  On step 4, specify the driver path like
     A:\CLIENT32\ND01XSRV.LAN , then following step  3..7  to complete the
     installation.


   C. Driver Installation Procedures on Client 32 for Windows 95 :
   ---------------------------------------------------------------
     If you have installed the Microsoft Client in your Windows 95 system,
     you should remove the adapter object & NDIS 2/3 driver of the ND01X
     adapter from the  Windows 95 system. If you have installed previously
     Unex's ND01X  NDIS 2/3 driver, you should do the following steps
     before installing the ND01X Client 32 driver. ( Note:  If you never
     pluged  Unex  ND01X  adapter into your PC, Procedure C.1 is not
     necessary.  And you just start from Procedure C.2)

     C.1 Remove the previously installed adapter object & driver of Unex
         ND01X, if any.
         -------------------------------------------------------------------
         1. Under Windows 95 system directory C:\WIN95\INF\, you should
            delete ND01XSRV.INF, *.BIN files.
         2. Click the "My Computer" icon in the Main Program Group.
         3. Click the "Control Panel" icon from My Computer window.
         4. Click the "System" icon from the Control Panel window.
         5. Click the "Device Manager" item.
         6. Click the "Network adapter" item from System window.
         7. Click the "Unex ND01X Fast Ethernet Adapter" icon from
             System window.
         8. Click <Remove> button, then click <OK> button.
         9. Close the opened windows.


     C.2 Driver Installation on Client 32 for Windows 95 :
     -----------------------------------------------------
         1. Plug Unex's ND01X adapter into your PC machine.
         2. Turn the power on to bootup the Windows 95.
         3. Windows 95 will then prompt the "Unex ND01X Fast Ethernet
            Adapter" in New Hardware Found dialog box.
         4. Following instructions to complete the installation, Window 95
            will ask you the proper path of the following diskette:

             a. Netware Client 32 for Windows 95 Disk
             b. Unex ND01X  Fast Ethernet Adapter Driver Diskette:
                Insert ND01X Driver Diskette, then, assign the path to
                A:\Client32
             c. Windows 95 CD-ROM

                                        -- Unex Technology Corporation --
