   LAN Server 4.0

   [1].Introduction:
   -------------
      This document describes the procedure to install NDIS driver on DOS
      LAN Requester and OS/2 LAN server 4.0 for Unex ND01X fast PCI
      ethernet adapter.

   Location of Driver:
        (diskette)
                \NDIS\DOS\ND01X.DOS  (for DOS LAN Services)
                \NDIS\OS2\ND01X.OS2  (for OS/2 LAN Server)
        (CD-ROM)
                \DRIVERS\NIC\ND01X\NDIS\DOS\ND01X.DOS (for DOS LAN Services)
                \DRIVERS\NIC\ND01X\NDIS\OS2\ND01X.OS2 (for OS/2 LAN Server)

   [2].Installing driver procedure on DOS LAN Requester :
   --------------------------------------------------
      Before you start with the installation  process,  make sure that
      DOS LAN Services is properly installed.  Similarly, your adapter
      should also be properly installed in your client PC.

      1. Copy ND01X.DOS from your Driver diskette (A:\NDIS\DOS)
         to DOS LAN Services subdirectory C:\DLS .

      2. Under DOS LAN Requester subdirectory C:\DLS, run INSTALL

      3. The  screen  display  some description. If it's correct, move
         highlight to "The listed options are correct" item ,then press
         ENTER.

      4. Move highlight to "Network Card", then press ENTER.

      5. Select "Change driver for network card." item, then press ENTER.

      6. Select "Network card not shown in list below..", then press ENTER.

      7. Insert the Unex ND01X driver diskette in floppy A,and specify
         your pathname A:\NDIS\DOS,then press ENTER.

      8. Unex ND01X driver is now installed on your computer, reboot
         your computer.


   [3].Installing driver procedure on OS/2 LAN Server 4.0:
   ---------------------------------------------------
      Before you start with the installation  process,  make sure that
      OS/2 LAN Server  is properly installed.  Similarly, your adapter
      should also be properly installed in your server.

      1. In OS/2 window, Click the "MPTS" icon.

      2. The screen will display the IBM Log, press "OK".

      3. Select "Install" button.

      4. Insert the Unex ND01X driver diskette, specify the driver
         path A:\NDIS\OS2 and press <Enter>.

      5. When complete above step to load  ND01X.OS2  into OS/2 system,
         then configure your system.

      6. The same step as step 3, select "Configure" button.

      7. The screen will display "Configure" dialog box and select "LAN
         adapters and protocols" then press "configure" button.

      8. The screen will display "LAPS Configuration" dialog box, move
         highlight to "ND01X Fast PCI Ethernet Adapter" item in "Network
         Adapter" window, and select "NetBios"  protocol. Press "OK".

      9. Installation is complete now. Reset your PC by turning it off
          and on.

    [4].Installing Multiple LAN Adapters:
    ----------------------------------
      1.follow [3]. 1-9 and add two ND01X Adapter driver

      2.in IBM Lan Services icon, OS/2 Lan Sercices Installation
                                                           /Configuration
        Select your the server of the insatlled,[OK].
        Do you want to re-install this version.[No].
        Installing tow card driver [OK] in mpts.
        Configure a component. [OK]
        Lan Services Adapters. [OK]
        Configure. [OK]
        Two Adapter [V]. OK


    [5].A sample PROTOCOL.INI file:
    -------------------------------

         [ND01X]
         DriverName=ND01X$
         EtherID=@52544C111111  ;This  keyword is used to desinate a ND01X
                                ;adapter by assigning it's ethernet ID
                                ;when more than one adapters exist on one
                                ; system.

         BusNo=@00          ;This  keyword is used to desinate a ND01X
                            ;adapter by assigning it's PCI bus number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'DeviceNo' keyword)

         DeviceNo=@0A       ;This  keyword is used to desinate a ND01X
                            ;adapter by assigning it's PCI Device number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'BusNo' keyword)

         Speed= 100/10      ;This keyword is used to force ND01X adapter
                            ;to speed 10M or 100M mode. If not present,
                            ;the driver will auto-detect the speed.




                                        -- Unex Technology Corporation --
