   Server Driver for NetWare 4.11

   Introduction:
   -------------
   This document describes the procedure to install the NetWare v4.11
   server driver for Unex ND01X Ethernet/Fast Ethernet PCI Bus adapter.

   Location of Driver:  \NWSERVER\41X\ND01XSRV.LAN (diskette) or
                        \DRIVERS\NIC\ND01X\NWSERVER\41X\ND01XSRV.LAN (CD-ROM)

   Installaton Procedure :
   ---------------------
      Before you start with the installation  process,  make sure that
      the Novell NetWare v4.11 server is properly installed.
      Similarly, your adapter should also be properly installed in your
      server.
      1. Insert the Unex Driver Diskette into drive A and check the
         contents of subdirectory  \NWSERVER\41X, It should contain the
         following file :

         ND01XSRV.LANÄÄÄ  Novell NetWare V4.11 Server Driver
         ND01XSRV.LDIÄÄÄ  Novell NetWare V4.11 Server Driver Installation
                        Information File

      2. At the  NetWare prompt (indicated by the Server name), run the
         INSTALL.NLM program by typing:

         server name: LOAD INSTALL <Enter>

      3. From Installation Options dialogue box, select "Driver options   
         (load/unload disk and network drivers)" and press <Enter>.

      4. From Driver Options dialogue box, select "Configure network
         drivers"  and press <Enter>.

      5. From Addition Driver Actions dialogue box, select "Select an
         additional driver" and press <Enter>

      6. Press the <Ins> key to specify other drivers to install.

      7. Press  <F3>  and specify the driver path (A:\NWSERVER\41X)
         and press <Enter>.

      8. The ND01XSRV.LAN driver should appear in your choice list for 
         the 'Select a driver to install' field. Choose this  driver to start
         the driver loading and  binding  procedure.  This will allow 
         you to load and bind all 4 frame types supported by NetWare.

      9. Add the LOAD and BIND statements you require to the server's
         AUTOEXEC.NCF file so that the LAN driver will load automatically
         each time the server starts up.


      Installation Notes:
      -------------------
      1.Installing Multiple LAN Adapters:
         The keyword  "SLOT"  is  provided for multiple LAN adapters in a
         single server by the driver ND01X.LAN.  So, add EtherID in LOAD
         commands. For example:

         LOAD ND01XSRV FRAME=Ethernet_802.2 NAME=LAN_A SLOT=1
         BIND IPX TO LAN_A NET=11
         LOAD ND01XSRV FRAME=Ethernet_802.2 NAME=LAN_B SLOT=2
         BIND IPX TO LAN_B NET=22

      2. The keyword  "SPEED"  is  provided for specifying adapter's speed
         (10M/100M), add SPEED in LOAD commands. For example:

         LOAD ND01XSRV FRAME=Ethernet_802.2 NAME=LAN_A SLOT=1 SPEED=100
         BIND IPX TO LAN_A NET=11

                                        -- Unex Technology Corporation --
