   LAN Manager Workstation/Server

   Introduction:
   -------------
   This document describes the procedure to setup LAN  Manager 2.1
   Workstation/Server driver for Unex ND01X Fast PCI ethernet adapter.

   Location of Driver:
   (diskette)
      (DOS) \MSLANMAN.DOS\DRIVERS\ETHERNET\ND01X\ND01X.DOS
      (OS/2)\MSLANMAN.OS2\DRIVERS\ETHERNET\ND01X\ND01X.OS2
   (CD-ROM)
      (DOS) \DRIVERS\NIC\ND01X\MSLANMAN.DOS\DRIVERS\ETHERNET\ND01X\ND01X.DOS
      (OS/2)\DRIVERS\NIC\ND01X\MSLANMAN.OS2\DRIVERS\ETHERNET\ND01X\ND01X.OS2


   Sample Configuration Files:
   ---------------------------
      CONFIG.SYS (for DOS will contain):

          DEVICE=C:\LANMAN.DOS\DRIVERS\PROTMAN\PROTMAN.DOS /I:C:\LANMAN.DOS
          DEVICE=C:\LANMAN.DOS\DRIVERS\ETHERNET\ND01X\ND01X.DOS


      CONFIG.SYS (for OS/2 will contain):

          DEVICE=C:\LANMAN.OS2\DRIVERS\PROTMAN\PROTMAN.OS2 /I:C:\LANMAN.OS2
          DEVICE=C:\LANMAN.OS2\DRIVERS\ETHERNET\ND01X\ND01X.OS2

          PROTOCOL.INI (will contain):


         [ND01X]
         ; ND01X RPOTOCOL.INI SAMPLE
         DriverName=ND01X$
         EtherID=@52544C111111  ;This  keyword is used to desinate a ND01X
                                ;adapter by assigning its ethernet ID
                                ;when more than one adapters exist on one
                                ; system.

         BusNo=@00          ;This  keyword is used to desinate a ND01X
                            ;adapter by assigning it's PCI bus number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'DeviceNo' keyword)

         DeviceNo=@0A       ;This  keyword is used to desinate a ND01X
                            ;adapter by assigning it's PCI Device number
                            ;when more than one adapters exist on one
                            ; system.(must be used with 'BusNo' keyword)

         Speed= 100/10      ;This keyword is used to force ND01X adapter
                            ;to speed 10M or 100M mode. If not present,
                            ;the driver will auto-detect the speed.



   Setup driver procedures on LAN Manager workstation/server :
   -----------------------------------------------------------
      Before you start with the installation process, make sure that the
      adapter  is properly  installed  and  configured. Make  sure  your
      Microsoft LAN Manager is properly installed.

      1. Run the appropriate Microsoft Lan Manager SETUP for computer you
         are setting up.(DOS, OS/2 or OS/2 Server). Select "Configuration"
         item ,(the Unex driver isn't included on the Lan Manager disk)
         and insert the Unex  ND01X  driver disk,  select the Unex
         driver and follow the directions.

      2. When completed, reboot your computer.


       Installing Multiple LAN Adapters:
   ----------------------------------

          To Follow Setup driver Procedure and add two adapter,

          Under  DOS  mode, you can modify the EtherID or BusNo+DeviceNo
          Keyword field in file C:\LANMAN\PROTOCOL.INI.


                                        -- Unex Technology Corporation --
