   Windows 95, OSR2

   Introduction:
   -------------
   This document describes the procedure to install  Windows 95 and OSR2
   driver for Unex ND01X PCI Fast Ethernet adapter.

   Location of Driver:  \WIN95\ND01XND3.SYS (diskette) or
                        \DRIVERS\NIC\ND01X\WIN95\ND01XND3.SYS (CD-ROM)

   Installing driver procedure on Microsoft Windows 95 :
   -----------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Windows 95, it will auto-detect your system configuration
      and find the adapter hardware.  ( If Win95 does not  prompt that it
      detects the PCI Ethernet adapter, there must be something wrong with
      the ND01X PCI Fast Ethernet adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select "Driver
         from disk provided by hardware manufacturer".

      2. Insert the Unex ND01X driver disk into drive A and specify
         the setup file pathname A:\Win95 .

      3. Windows 95 will appear some messages to insert Windows 95 system
         disk to complete setup step.

      4. Windows 95  will  finish  the  other  installation  procedure
         automatically, then you restart the system.


                                        -- Unex Technology Corporation --
